**NOTES: UNLESS OTHERWISE SPECIFIED.**

1. APPLICABLE STANDARDS/SPECIFICATIONS:

ASME Y14.3-2012, ORTHOGRAPHIC AND PICTORIAL VIEWS.

ASME Y14.5-2009, DIMENSIONS AND TOLERANCES.

ASME Y14.38.-2013, ABBREVIATIONS AND ACRONYMS.

1. ALL DIMENSIONS ARE IN MILLIMETERS.
2. MATERIAL: 125 MICRONS MATTE POLYCARBONATE (LEXAN 8B35) SUBSURFACE PRINT.
3. COLOR/TINTS: BLACK PANTONE 2C, COOL GREY PANTONE 6C.
4. ADHESIVE: PRESSURE SENSITIVE ADHESIVE (3M467)
5. SCREEN PRINTING PER ARTWORK 10073068 REV D. ARTWORK FOR REFERENCE ONLY.
6. PRINT AS PER LOCAL MANUFACTURING PROCEDURES. CENTER ARTWORK ON LABEL.
7. ALCOHOL RESISTANT INK.
8. PART/COMPONENT TO BE RoHS COMPLIANT.

